[bookmark: grc_façade_inspection_checklist]GRC Façade Inspection Checklist
Use this checklist as a printable or digital aid when inspecting and maintaining glass reinforced concrete (GRC/GFRC) cladding systems. Adapt frequencies to your asset-management plan.
[bookmark: bm_1_pre_task_planning]1. Pre-task planning
· [ ] Method statement prepared and approved
· [ ] Task briefing completed with all operatives
· [ ] Lifting plan and access strategy defined
· [ ] Required permits obtained from asset/station operator
· [ ] Hoarding / barriers planned where works occur near the public
[bookmark: bm_2_access_and_safety]2. Access and safety
· [ ] Appropriate access equipment selected (MEWP, scaffold tower, lifting robot, mini crane)
· [ ] Access equipment inspected and within certification dates
· [ ] Working-at-height training verified for all operatives
· [ ] Fall-protection and safety tethers available where required
· [ ] Escalators or sensitive assets protected before tower erection
[bookmark: bm_3_routine_visual_inspection_of_4dd94a]3. Routine visual inspection of GRC panels
· [ ] All visible panels checked for looseness or insecurity
· [ ] Panels checked for misalignment or displacement
· [ ] Surface staining, grease or oil contamination identified
· [ ] Dust build-up and general soiling recorded
· [ ] Graffiti or impact damage noted
· [ ] Interfaces with adjacent architectural elements inspected
[bookmark: bm_4_substructure_fixings_and_anchors]4. Substructure, fixings and anchors
· [ ] Steel substructure inspected for deformation or damage
· [ ] Brackets, rails and stud sections checked for corrosion
· [ ] Mechanical fixings (bolts, screws, connectors) checked for looseness
· [ ] Safety tethers and locking mechanisms inspected
· [ ] Concrete anchors visually inspected where accessible
· [ ] Anchor pull-out tests carried out where specified
[bookmark: bm_5_hidden_components_insulation_3788ad]5. Hidden components: insulation and smoke barriers
· [ ] Acoustic insulation condition checked where panels are removed
· [ ] Horizontal smoke barriers inspected and intact
· [ ] Vertical smoke barriers inspected and intact
· [ ] Any damaged or missing barriers scheduled for repair/replacement
[bookmark: bm_6_cleaning_operations]6. Cleaning operations
· [ ] Cleaning method selected (hand-wipe, brush, pole system)
· [ ] Only approved cleaning agents used (e.g. lukewarm soapy water)
· [ ] Bleaches, abrasive cloths or harsh detergents explicitly excluded
· [ ] Passenger-interface panels cleaned at agreed frequency
· [ ] High-level panels cleaned according to site-specific needs
· [ ] Deep-clean schedule (every 2–5 years) reviewed and updated
[bookmark: bm_7_panel_repair_and_replacement]7. Panel repair and replacement
· [ ] Minor chips and edge defects assessed for repair
· [ ] Repair mix / kit available and compatible with GRC system
· [ ] Perforations or holes patched using appropriate tools
· [ ] Sanding and finishing carried out to acceptable visual standard
· [ ] Panels scheduled for removal/replacement identified
· [ ] Removal and reinstallation procedures followed step-by-step
[bookmark: bm_8_escalator_and_complex_geometries]8. Escalator and complex geometries
· [ ] Special access arrangements planned for escalator shafts and tight spaces
· [ ] Panels in complex geometries inspected for movement and damage
· [ ] Any bespoke fixings or brackets checked and documented
[bookmark: bm_9_testing_and_qa]9. Testing and QA
· [ ] Torque checks completed on critical screws and bolts
· [ ] Test results recorded against asset IDs or panel references
· [ ] Inspection and test plans (ITPs) updated where applicable
[bookmark: bm_10_documentation_and_reporting]10. Documentation and reporting
· [ ] Inspection findings recorded in a written report
· [ ] Photos taken of defects, repairs and critical components
· [ ] Outstanding actions assigned with deadlines and responsibilities
· [ ] Maintenance history updated in asset-management system
